## Macro Command Reference

`aformat <AXIS> <AXISFORMAT>`

Defines the axis format.

`AXIS`

Defines the axis to which the command apply. Possible values are:

`all` | all four axis
`x` | both X axis
`y` | both Y axis
`1, x1, xb, bottom` | 1. X axis (bottom)
`2, y1, yl, left` | 1. Y axis (left)
`3, x2, xt, top` | 2. X axis (top)
`4, y2, yr, right` | 2. Y axis (right)

`AXISFORMAT`

The axis format:

`0, lin` | linear axis
`1, log` | logarithmic axis
`2, time` | time axis
`3, bin` | binary axis with base 2 numbers