## Macro Command Reference

`asetreverse <AXIS> <BOOL>`

If set the axis will be reverse plotted.

`AXIS`

Defines the axis to which the command apply. Possible values are:

`all` | all four axis
`x` | both X axis
`y` | both Y axis
`1, x1, xb, bottom` | 1. X axis (bottom)
`2, y1, yl, left` | 1. Y axis (left)
`3, x2, xt, top` | 2. X axis (top)
`4, y2, yr, right` | 2. Y axis (right)

`BOOL`

this is a switch parameter which can only have two values.Possible values:

`0, false, no, off` | Switch On
`1, true, yes, on` | Switch Off