## Macro Command Reference

`anumalign <AXIS> <ALIGN>`

Defines the alignment of axis numbers.

`AXIS`

Defines the axis to which the command apply. Possible values are:

`all` | all four axis
`x` | both X axis
`y` | both Y axis
`1, x1, xb, bottom` | 1. X axis (bottom)
`2, y1, yl, left` | 1. Y axis (left)
`3, x2, xt, top` | 2. X axis (top)
`4, y2, yr, right` | 2. Y axis (right)

`ALIGN`

A parameter wich defines the alignment of different objects, possible values:

`topleft tl 1` | `topcenter tc 2` | `topright tr 3`
`centerleft cl 8` | `center c 0` | `centerright cr 4`
`bottomleft bl 7` | `bottomcenter bc 6` | `bottomright br 5`