## Macro Command Reference

`atickdist <AXIS> <dist>`

Defines the distance between two major ticks. If your axis is a time axis you have to enter `days:hours:minutes:seconds` or `w` (1 week) or `m` (1 month) or `y` (1 year).

`AXIS`

Defines the axis to which the command apply. Possible values are:

`all` | all four axis
`x` | both X axis
`y` | both Y axis
`1, x1, xb, bottom` | 1. X axis (bottom)
`2, y1, yl, left` | 1. Y axis (left)
`3, x2, xt, top` | 2. X axis (top)
`4, y2, yr, right` | 2. Y axis (right)