## Macro Command Reference

`copydata <subview number> [RANGE]`

Copy data from one subview to the current. If no range is given all data buffers will be copied.

`RANGE`

A list of numbers (e.g. used for the `loop` command):

`n` | defines a range from 0 to n
`from;to;step` | defines a range where the arguments may be math expressions.
`b1,b2,b3,...,bn` | a list of numbers where the arguments may be math expressions.
`bs..be` | numbers from bs to be