## Macro Command Reference

`aexpoffset <AXIS> <offset>`

Allows you to define the limit, above which numbers are plotted in exponential notation. The number you define is the exponent of the limit.

`AXIS`

Defines the axis to which the command apply. Possible values are:

`all` | all four axis
`x` | both X axis
`y` | both Y axis
`1, x1, xb, bottom` | 1. X axis (bottom)
`2, y1, yl, left` | 1. Y axis (left)
`3, x2, xt, top` | 2. X axis (top)
`4, y2, yr, right` | 2. Y axis (right)